
NAME:  AESGW22-8 Eight Spindle Motor Coil Winding Machine      
Specifications：

	Spindle number
	8

	Wire size range
	0.1-0.5mm

	Loop diameter
	260mm

	Max wire distance
	9.99mm

	Winder width
	180mm

	Max speed
	0-3500 RPM

	Spindle motor
	Three Phase motor AC Drive

	Winder motor
	Stepping motor

	Input power
	220V  50HZ/60HZ

	Machine size
	1320×900×1320mm

	Package size
	1630×1050×1520mm

	N/G weight
	200kg/442kg


Features:

There have eight pcs winding head, the winding head length and elevation can be easily adjusted.

Equipped with mobile wire frame (including eight  group bobbin and eight spools ,size is  120mm × 300mm diameter ).

Install brake resistors, the position more accurately
Multi spindle coil winding machine design of 32 bit controller chip, It’ll be faster, and higher reliability.

In Chinese and English display,easy to operation,winding data retention after power failure, not to discarded products。

All the parts for multi spindle coil winding machine are imported prats,such as:Japan Bearing (NSK、NTN),Japan BANDO belt ，U.S.A GATES belt ，Taiwan Ball screw (TBI)，Taiwan Transducers and so on.

Change the winding spindle is by pneumatic . 

Eight Spindle Motor Coil Winding Machine can be used for multi connected, coil automatic wire winding of multilayer type , it can winding  1-8 wire at one time.

Coil winding machine can also be pass the groove automatically . 

Coil winding machine can winding 1-32 coils in the winder length range. 

There are two alternate use of the square shaft rotatable about the coil diameter 25MM-180MM, high production efficiency.

For the characteristics of the machine winding ,the machine body use thick cast iron , The vibration and noise of smaller machines, it also have when wire cutting the machine will stop function, not discarded products.

Multi spindle coil winding machine can winding a variety of motor coil product, including industrial motors, air conditioner motors, washing machine motors, fan motors,Fishing line spool product.
Advantages:

There have eight pcs winding head, the winding head length and elevation can be easily adjusted.

Equipped with mobile wire frame (including eight  group bobbin and eight spools ,size is  120mm × 300mm diameter ).

With two mold spindle :dimensions 16 × 16 × 630mm 

Supply frame  size is 800 × 800 × 780mm.

Install brake resistors, the position more accurately 

PRODUCT:
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APPLICATION:

Toroid Winding Machine is the best suited to toroidal inductor, toroidal transformers,toroidal current transformers,toroidal coil, toroid choke coil, power inductors,UPS inductor,converter inductor and heavy toroidal core etc. 
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PRACTICAL APPLICATION :

TRAINNING CUSTOMER TO OPERATE WINDING MACHNE :
1.All service engineers with 10 years experience are gotten special technology training, who can deal with various breakdown problem.
2.Guide the user to use accurately and how to maintain the Eight Spindle Motor Coil Winding Machine    .
Provide free consultation about production process technology of electronic Eight Spindle Motor Coil Winding Machine .
3.In order to guarantee the machine used normally, we'd have training on how to operate, use and maintain our product by English manual, video, guiding on line.
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PACKAGING:

Packaging Material: Carton/Wooden case with foam inside.
1.General package(Paper carton or plastic bag): For small euipped parts for Eight Spindle Motor Coil Winding Machine      

, Package it with form and pack paper to guarantee unbroken during the transport.
2.Wooden case package: For larger scale Eight Spindle Motor Coil Winding Machine ,we have special skilled carpenter, who would make the proper wooden case with exact thickness,density,length. The up arrow ↑marked on the  outer wooden case. Buffer material would be put in the wooden case to prevent crack and shock.
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FACTORY:

We-GREWIN INDUSTRIAL GROUP is expert in winding machines lines for 28Years. Our Grewin have ISO9001:2015,CE approvals,Machines'Patents,"high-tech enterprises"by the government.
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